( TL19E20A14400049001KBAT00 )

Radiator Replacement

1. Drain the engine coolant.

1. Raise the vehicle on the lift to full height.

1. Remove the splash shield.

1. Remove the lower radiator hose (A).

1. A/T model: Remove the automatic transmission fluid (ATF) cooler hoses (B), then plug the hose and line.

1. Disconnect the fan motor connectors (C) and engine coolant temperature (ECT) sensor 2 connector (D), then remove the harness clamps (E).

1. Lower the vehicle on the lift.

1. Remove the grille cover.