( TL19E20A32200043711KCAT00 )

Engine Oil/Air Separator Installation

1. Remove all of the old liquid gasket from the oil/air separator mating surfaces, bolts, and bolt holes.

1. Clean, and dry the oil/air separator mating surfaces.

1. Apply liquid gasket (P/N 08C70-K0234M, 08C70-K0334M, or 08C70-X0331S) to the engine block mating surface of the oil/air separator and to the inner threads of the bolt holes.
   NOTE:
   - Apply liquid gasket about 2.5 mm (0.098 in.) diameter bead along the broken line (A).
   - Do not install components if 5 minutes or more have passed after applying the liquid gasket. Instead, remove the old residue and reapply the liquid gasket.

1. Install the oil/air separator.
   NOTE:
   - Wait at least 30 minutes before filling the engine with oil.
   - Do not run the engine for at least 3 hours after installing the oil/air separator.