( TL19E00J16126721301KBAT00 )

Front Door Outer Handle Replacement

With Super Locking
NOTE: Put on gloves to protect your hands.

1. Remove these items:
   - Tweeter cover
   - Door panel
   - Door end trim

1. Raise the glass fully.

1. Disconnect the power door lock actuator connector (A).

1. Remove the rear plug cap (B), then remove the plastic cover (C) as needed.
   NOTE: Remove the glue from the door surface. If the plastic cover is damaged or torn, replace it.