( TL19E20A14674300000KAAT00 )

Cam Chain Removal

NOTE: Keep the cam chain away from magnetic fields.

1. Remove the front wheels.

1. Remove the splash shield.

1. Remove the drive belt auto-tensioner.

1. Remove the cylinder head cover.

1. Set the No. 1 piston at top dead center (TDC). The ‘‘UP'' mark (A) on the camshaft sprocket should be at the top, and the TDC grooves (B) on the camshaft sprocket should line up with the top edge of the head.