( TL19E00J34200057269MBAT00 )

Sunroof Glass Position Adjustment

The roof panel (A) should be even with the glass weatherstrip (B), to within 0+1/−1 mm (0+0.04/−0.04 in.) all the way around, and the weatherstrip should evenly touches the roof panel in its front and rear. If not, make the following adjustment: |

1. Remove the bracket cover.

1. Adjust the glass (A).

   -1. | Using a TORX T25 bit, slightly loosen the bolts.
   -2. | Move the glass up or down and forward or rearward.
   -3. | Tighten all bolts securely.

1. If necessary, repeat on the opposite side.

1. Reset the sunroof control unit.