( TL19E00J26216516402KDAT00 )

Center Console Armrest Removal/Installation

1. With rear ventilation: If necessary, remove the screws, then remove the rear duct (A) from behind the console box (B).

1. Install the armrest in the reverse order of removal, and note these items:
   - Replace the E-clips with new ones.
   - Apply low strength liquid thread lock to the 5 mm screws fastening the opening spring and both the side panels before reinstallation.
   - Make sure the ribs of the driver's side panel and the passenger's side panel are engaged to the hooks of the console box securely.