( TL19E00K761000N1306FAAT00 )

DTC Troubleshooting: 1306

DTC 1306:
Vehicle Speed Pulse
NOTE:

- Check the vehicle battery condition first.
- Before you troubleshoot, make sure to follow the general troubleshooting information.

1. Clear the hard error code.

1. Turn the ignition switch to LOCK (0), and then start the engine.

1. Check for the hard error code.

Is DTC 1306 indicated?

YES | - | Go to Step 4 .
NO | - | Intermittent failure, the system is OK at this time.■

1. Drive the vehicle and watch the VSP signal.

Does the VSP signal change from [0] to [1] as you drive?

YES | - | Replace the navigation unit. ■
NO | - | Do the symptom troubleshooting for Vehicle position icon constantly leaves road, moves erratically or is very far from actual position. ■