( TL19E3PK77100090723FAAT00 )

DTC Troubleshooting: P0723 (9)

DTC P0723:
Output Shaft (Countershaft) Speed Sensor Intermittent Failure
NOTE:

- Before you troubleshoot, record all freeze data and any on-board snapshot with the HDS, and review General Troubleshooting Information.
- This code is caused by an electrical circuit problem and cannot be caused by a mechanical problem in the transmission.

K24Z3 Engine Model

1. Turn the ignition switch to ON (II).

1. Clear the DTC with the HDS.

1. Test-drive the vehicle with the shift lever in D, with the engine speed above 2,000 rpm (min −1 ), and let the transmission shift through all five gears.

1. Monitor the OBD STATUS for P0723 in the DTCs MENU with the HDS.

Does the HDS indicate FAILED?

YES | - | Go to Step 5 .
NO | - | If the HDS indicates PASSED, intermittent failure, the system is OK at this time. Check for poor connections or loose terminals between the output shaft (countershaft) speed sensor and the PCM. If the HDS indicates NOT COMPLETED, go to Step 3 .

1. Turn the ignition switch to LOCK (0).

1. Disconnect the output shaft (countershaft) speed sensor connector, and inspect the connector and connector terminals to be sure they are making good contact.

Are the connector terminals OK?

YES | - | Go to Step 7 .
NO | - | Repair the connector terminals, then go to Step 7 .

1. Connect the output shaft (countershaft) speed sensor connector.

1. Test-drive the vehicle with the shift lever in D, with the engine speed above 2,000 rpm (min −1 ), and let the transmission shift through all five gears.

1. Monitor the OBD STATUS for P0723 in the DTCs MENU with the HDS.

Does the HDS indicate FAILED?

YES | - | Go to Step 10 .
NO | - | If the HDS indicates PASSED, troubleshooting is complete. If the HDS indicates NOT COMPLETED, go to Step 8 .

1. Turn the ignition switch to LOCK (0).

1. Jump the SCS line with the HDS.

1. Disconnect PCM connector C (49P).

1. Check for continuity between PCM connector terminal C44 and body ground, and between terminal C48 and body ground.

Is there continuity?

YES | - | Go to Step 14 .
NO | - | Repair open in the wires between PCM connector terminals C44, C48, and body ground (G101), or repair poor ground (G101), then go to Step 33 .

1. Connect PCM connector C (49P).

1. Disconnect the output shaft (countershaft) speed sensor connector.

1. Turn the ignition switch to ON (II).

1. Measure the voltage between output shaft (countershaft) speed sensor connector terminal No. 1 and body ground.

Is there about 5 V?

YES | - | Go to Step 18 .
NO | - | Go to Step 29 .

1. Turn the ignition switch to LOCK (0).

1. Jump the SCS line with the HDS.

1. Disconnect PCM connector B (49P).

1. Check for continuity between output shaft (countershaft) speed sensor connector terminal No. 2 and body ground.

Is there continuity?

YES | - | Repair short to body ground in the wire between PCM connector terminal B38 and the output shaft (countershaft) speed sensor, then go to Step 33 .
NO | - | Go to Step 22 .

1. Connect PCM connector B (49P).

1. Turn the ignition switch to ON (II).

1. Measure the voltage between output shaft (countershaft) speed sensor connector terminal No. 2 and body ground.

Is there about 5 V?

YES | - | Replace the output shaft (countershaft) speed sensor, then go to Step 33 .
NO | - | Go to Step 25 .

1. Turn the ignition switch to LOCK (0).

1. Jump the SCS line with the HDS.

1. Disconnect PCM connector B (49P).

1. Check for continuity between PCM connector terminal B38 and output shaft (countershaft) speed sensor connector terminal No. 2.

Is there continuity?

YES | - | Go to Step 39 .
NO | - | Repair open in the wire between PCM connector terminal B38 and the output shaft (countershaft) speed sensor, then go to Step 33 .

1. Turn the ignition switch to LOCK (0).

1. Jump the SCS line with the HDS.

1. Disconnect PCM connector C (49P).

1. Check for continuity between PCM connector terminal C13 and output shaft (countershaft) speed sensor connector terminal No. 1.

Is there continuity?

YES | - | Go to Step 39 .
NO | - | Repair open in the wire between PCM connector terminal C13 and the output shaft (countershaft) speed sensor, then go to Step 33 .

1. Reconnect all connectors.

1. Turn the ignition switch to ON (II).

1. Clear the DTC with the HDS.

1. Test-drive the vehicle at speeds over 20 km/h (12 mph) with the shift lever in D, and let the transmission shift through all five gears.

1. Check for Temporary DTCs or DTCs with the HDS.

Is DTC P0723 indicated?

YES | - | Check for poor connections or loose terminals between the output shaft (countershaft) speed sensor and the PCM, then go to Step 1 .
NO | - | Go to Step 38 .

1. Monitor the OBD STATUS for P0723 in the DTCs MENU with the HDS.

Does the HDS indicate PASSED?

YES | - | Troubleshooting is complete. If any other Temporary DTCs or DTCs were indicated in Step 37 , go to the indicated DTC's troubleshooting.■
NO | - | If the HDS indicates FAILED, check for poor connections or loose terminals between the output shaft (countershaft) speed sensor and the PCM, then go to Step 1 . If the HDS indicates NOT COMPLETED, go to Step 36 .

1. Reconnect all connectors.

1. Update the PCM if it does not have the latest software, or substitute a known-good PCM.

1. Test-drive the vehicle at speeds over 20 km/h (12 mph) with the shift lever in D, and let the transmission shift through all five gears.

1. Check for Temporary DTCs or DTCs with the HDS.

Is DTC P0723 indicated?

YES | - | Check for poor connections or loose terminals between the output shaft (countershaft) speed sensor and the PCM. If the PCM was updated, substitute a known-good PCM, then go to Step 41 . If the PCM was substituted, go to Step 1 .
NO | - | Go to Step 43 .

1. Monitor the OBD STATUS for P0723 in the DTCs MENU with the HDS.

Does the HDS indicate PASSED?

YES | - | If the PCM was updated, troubleshooting is complete. If the PCM was substituted, replace the original PCM. If any other Temporary DTCs or DTCs were indicated in Step 42 , go to the indicated DTC's troubleshooting.■
NO | - | If the HDS indicates FAILED, check for poor connections or loose terminals between the output shaft (countershaft) speed sensor and the PCM. If the PCM was updated, substitute a known-good PCM, then go to Step 41 . If the PCM was substituted, go to Step 1 . If the HDS indicates NOT COMPLETED, go to Step 41 .