( TL19E00D14300014804KBAT00 )

Brake Pedal Cover Replacement

NOTE: This procedure shows a model equipped with a metal brake pedal cover.

1. Cover the carpet under the brake pedal to prevent metal shavings from getting on the carpet.

1. Center-punch each of rivets (A), and drill their heads off with a 3 mm (0.12 in.) drill bit (B).
   NOTE: Do not drill the brake pedal pad (C).

1. Remove the brake pedal plate (A) and the brake pedal cover (B) from the brake pedal pad (C).

1. Set the brake pedal cover to the brake pedal plate.

1. Install the brake pedal plate (A) with the rivets (B) firmly.

1. Make sure the brake pedal cover and plate is securely fastened on the brake pedal.

1. Check the brake pedal height.