( TL19E00G24100057401FEAT00 )

Sunlight Sensor Test

1. Remove the sunlight sensor (A).

1. Turn the ignition switch to ON (II). Measure the voltage between the terminals with the (+) probe on the No. 1 terminal and the (−) probe on the No. 2 terminal with the connector connected.
   NOTE: The voltage readings will not change under the light of a flashlight or a fluorescent lamp. Voltage should be:
   - 3.6−3.7 V or more with the sensor out of direct sunlight.
   - 3.3−3.5 V or less with the sensor in direct sunlight.

1. If the voltage is not as specified, replace the sunlight sensor.