( TL19E00J26273413801KDAT00 )

Interior Trim Removal/Installation - Pillar Areas

1. Reinstall the front pillar trim (A).

   -1. | Insert the bottom of the trim into the dashboard (B).

   -2.

   Place the trim over the front pillar (C), and fit its upper clip (D), the lower clip, and the pin (E) into the holes (F) in the front pillar, then lightly push the trim into place.
   NOTE:
   - Make sure the side curtain airbag isn't tucked down under the clips and the ribs.
   - Apply pressure to the areas of the trim on the upper clip until these clip fittings are felt. If you push too hard, the clip will be damaged, and it will not hold the trim properly.
   - Make sure the upper clip portions of the trim don't come off the body by tugging on the trim.

1. Reinstall the door opening seal.