( TL19E1AE34116317041MBAT00 )

Clutch Pedal, Clutch Pedal Position Switch, and Clutch Switch (SIL) Adjustment

1. Loosen the clutch switch (SIL) locknut (A).

1. Adjust the clutch switch (SIL) (B), so that the switch should be ON/OFF at the clutch switch (SIL) switch ON/OFF height (C).

   C | Clutch Switch (SIL) ON/OFF Height:
   | LHD model: | 94.6−97.1 mm (3.72−3.82 in.)
   | RHD model: | 91.4−93.9 mm (3.60−3.70 in.)

1. Tighten the clutch switch (SIL) locknut while holding the clutch switch (SIL).

1. Check the clutch operation.

1. Connect the clutch pedal position switch connector and the clutch switch (SIL) connector (if equipped), then check the cruise control and the shift indicator lamp operation.