( TL19E00E16236500000LDAT00 )

Intermediate Shaft Reassembly

Exploded View - R20A3 Engine Model
Exploded View - K24Z3 Engine Model
Special Tools Required
Oil seal driver, 64 mm
07GAD-PH70201
Half shaft base
07NAF-SR30101
Bearing driver attachment, 52 x 55 mm
07746-0010400
Inner bearing driver attachment, 35 mm
07746-0030400
Driver handle, 15 x 135L
07749-0010000
Installer attachment, 45 mm
07MAD-PR90100
NOTE:

- Refer to the Exploded View, as needed, during this procedure.
- The illustrations show K24Z3 engine model.

1. Clean the disassembled parts with solvent, and dry them with compressed air.
   NOTE: Do not wash the rubber parts with solvent.

1. Press a new intermediate shaft bearing (A) into the bearing support (B) using the 52 x 55 mm bearing driver attachment (C), the 15 x 135L driver handle (D), the half shaft base (E), and a press.