( TL19E00J54400049593KBAT00 )

Rain Sensor Cover Base Replacement

With Automatic Wiper
NOTE:

- Wear eye protection while cutting the glass adhesive with piano wire.
- LHD model is shown; RHD model is symmetrical.

1. Remove these items:
   - Headliner
   - Rain sensor
   - Rearview mirror

1. Carefully cut through the adhesive tape under the rain sensor cover base using the piano wire, then remove the base.
   NOTE: Take care not to damage the optical connector.

1. Use a putty knife to scrape off all of the old adhesive tape from the windshield. Clean the inside face of the windshield with isopropyl alcohol where new rain sensor cover is to be applied. Make sure the installing surface is kept free of water, oil and grease.

1. Apply primer on the double sided adhesive tape (A) of the rain sensor cover base (B). Let the primer dry at least 10 minutes, then attach it to the windshield with in 12 hours.

1. Attach the rain sensor cover base with adhesive tape to the inside face of the windshield as shown, then press the adhesive portions into place securely.
   NOTE: Without lane keep assist system: Be sure the rain sensor cover base lines up with the alignment marks (C).

1. Reinstall all remaining removed parts.

Without lane keep assist system
With lane keep assist system