( TL19E00J26216516409KDAT00 )

Center Console Panel Removal/Installation

1. Install the console panel in the reverse order of removal, and note these items:
   - Make sure each connector is plugged in properly.
   - If the clips are damaged or stress-whitened, replace them with new ones.
   - Push the clips and the hook into place securely.
   - Type-S: Install the shift knob in numbered sequence.

   - | Turn the spacer (A) until spacer contacts with shaft (B).
   - | Turn the shift knob (C) until shift knob contacts with spacer.
   - | Tighten the spacer when the shift pattern turn to front of vehicle, by turning back knob (amount of turning back: 360 ° MAX).