( TL19E00K766000U0155FAAT00 )

DTC Troubleshooting: U0155

DTC U0155:
Power Seat Control Unit Lost Communication with Gauge Control Module

1. Clear the DTCs with the HDS.

1. Turn the ignition switch to LOCK (0) and then back to ON (II).

1. Wait for 6 seconds or more.

1. Check for DTCs with the HDS.

Is DTC U0155 indicated?

YES | - | Go to Step 5 .
NO | - | Intermittent failure, the system is OK at this time. Check for loose or poor connections between the power seat control unit and the gauge control module.■

1. From the BODY ELECTRICAL system select menu, select UNIT INFORMATION, and then select CONNECTED UNIT.

Is the gauge control module detected?

YES | - | Replace the power seat control unit .■
NO | - | Go to Step 6 .

1. Turn the ignition switch to LOCK (0).

1. Disconnect the gauge control module 32P connector.

1. Disconnect power seat control unit connector A (40P).

1. Check for continuity between power seat control unit connector A (40P) No. 39 and No. 40 terminals and the gauge control module 32P connector No. 23 and No. 24 terminals individually.

Is there continuity?

YES | - | Replace the gauge control module .■
NO | - | An open in the wire between the gauge control module and the power seat control unit.■