( TL19E00D14300014791MDAT10 )

Front Brake Pad Inspection and Replacement

Replacement - 2-piston caliper type

1. Remove some brake fluid from the master cylinder.

1. Raise the front of the vehicle, and support it with safety stands in the proper locations.

1. Remove the front wheels.

1. Remove the brake hose mounting bolt (A).

1. Remove the flange bolt (B), and pivot the caliper (C) up out of the way. Check the hose and pin boots for damage and deterioration.