( TL19E00J32133100000FAAT00 )

HID Lamp System Troubleshooting

1. Check for continuity between the No. 1 terminal of the HID unit 2P connector and body ground.

Is there continuity?

YES | - | Replace the HID unit, then go to Step 15 .
NO | - | Repair open in the wire between the HID unit and body ground. If the wire is OK, check for poor ground (G201/G302), then go to Step 15 .

1. Do the battery terminal reconnection procedure.