( TL19E00D14300014791MDAT20 )

Rear Brake Pad Inspection and Replacement

1. Install the caliper into position. Install the flange bolts (A), and tighten it to the specified torque. While holding the caliper pin (B) with a wrench. Be careful not to damage the pin boots.

1. Clean the mating surfaces of the brake disc/drum and the inside of the wheel, then install the rear wheels.

1. Press the brake pedal several times to make sure the brakes work.
   NOTE: Engagement may require a greater pedal stroke immediately after the brake pads have been replaced as a set. Several applications of the brake pedal will restore the normal pedal stroke.

1. Add brake fluid as needed.

1. After installation, check for leaks at hose and line joints or connections, and retighten if necessary.
   Test-drive the vehicle, then recheck for leaks.