( TL19E00J10300000000CAAT10 )

USB Adapter Unit for Inputs and Outputs (Without Navigation System)
USB Adapter Unit Connector A (14P)

Cavity | Wire | Connects to
--- | --- | ---
A1 | WHT | Audio unit (+B)
A2 | LT BLU | Audio unit (SYS ON)
A3 | GRY * | Audio unit (GA-NET BUS SH)
A4 | GRY * | Audio unit (AUDIO SH)
A5 | GRN | Audio unit (AUDIO R+)
A6 | BLK | Audio unit (AUDIO L+)
A9 | RED | Audio unit (GA-NET BUS +)
A10 | GRN | Audio unit (GA-NET BUS −)
A11 | BLK | Audio unit (GND)
A13 | WHT | Audio unit (AUDIO R−)
A14 | RED | Audio unit (AUDIO L−)

*: | The shielded wires have a heat-shrunk tube insulating the outside of the wire. The color of the insulating tube, typically black or dark gray, may not match the color of the wire shown on the circuit diagram.

USB Adapter Unit Connector B (5P)

Cavity | Wire | Connects to
--- | --- | ---
B1 | ——— | USB Jack (USB V BUS)
B2 | ——— | USB Jack (USB DATA−)
B3 | ——— | USB Jack (USB DATA+)
B4 | ——— | USB Jack (USB GND)
B5 | ——— | USB Jack (USB SH)