( TL19E1PE10400013001MAAT00 )

ATF Level Check

1. If necessary, fill the transmission with ATF through the ATF dipstick guide tube opening (A) to bring the fluid level between the upper mark and the lower mark of the ATF dipstick. Do not fill the fluid above the upper mark. Always use genuine Honda ATF-Z1 automatic transmission fluid (ATF). Using a non-Honda ATF can affect shift quality.

1. Insert the ATF dipstick into the ATF dipstick guide tube aligning the notch with the guide tab.