( TL19E00D14300014791MDAT10 )

Front Brake Pad Inspection and Replacement

1. Apply Plastilube to the areas indicated by the arrows. Wipe excess grease off the brake pads (A). Keep grease off the brake discs and the brake pads. Contaminated brake discs or the brake pads reduce stopping ability.

1. Install the inner pad to the caliper body (B), and install the outer pad to the caliper bracket (C). If you are reusing the brake pads, always reinstall the brake pads in their original positions to prevent a momentary loss of braking efficiency.

Inner pad
Outer pad