( TL19E1AE34151150941FEAT00 )

M/T Reverse Lockout Solenoid Test

1. Remove the reverse lockout solenoid.

1. Connect battery positive terminal to the reverse lockout solenoid 2P connector terminal No. 2, and connect the battery negative terminal to the reverse lockout solenoid 2P connector terminal No. 1.

1. Make sure the reverse lockout solenoid works. If the reverse lockout solenoid does not work, replace it.
   NOTE: The inhibitor should be pushed out when applying the current to the solenoid, and the inhibitor shouled be released when no applying the current to the solenoid.