( TL19E1PE10411354171MAAT00 )

A/T Secondary Shaft 1st Gear Axial Clearance Inspection

Special Tools Required
Bearing driver attachment 42 mm
07QAD-P0A0100

1. Install the thrust needle bearing (A), the needle bearing (B), 1st gear (C), the thrust needle bearing (D), the 40 x 51.5 mm thrust washer (E), the 1st/3rd clutch (F), and the 3rd gear collar (G) on the secondary shaft (H). Do not install the O-rings during inspection.

1. Install the idler gear (I), then install the transmission housing bearing (J) on the idler gear using the 42 mm bearing driver attachment and a press.

1. Install the conical spring washer (K) and the locknut (L), then tighten the locknut to 29 N·m (3.0 kgf·m, 22 lbf·ft).