( TL19E00J26220200000KBAT00 )

Dashboard Replacement

1. Remove the screws, then remove the dashboard center stay (A) from the dashboard (B).

1. Remove the passenger's airbag.

1. Assemble the dashboard and the steering hanger beam in the reverse order of removal, and note these items:
   - Replace the passenger's airbag mounting bolts with new ones.
   - Make sure the dashboard fits onto the guide pins correctly.
   - Make sure the dashboard wire harness, the audio wire harness, and the antenna sublead are routed properly and not pinched.
   - Make sure each connector is plugged in properly.
   - Push the harness clips and the connector clip into place securely.
   - Do the battery terminal reconnection procedure
   - Check for any DTCs that may have been set during repairs, and clear them.
   - A/T model: If necessary, adjust the shift cable