( TL19E00R311000K5352YDAT07 )

Roof Panel Removal

NOTE: This section explains the procedures after removal of all accessories and related parts. For accessories' and related parts' removal procedure, refer to the appropriate Shop Manual.
Mass production body welding position and number (Roof panel, roof rail and roof arch A)
NOTE:

- Welding symbols
  : 2-Plate spot welding/ : 3-Plate spot welding/ : 4-Plate spot welding/ : MIG plug welding/ : MIG welding L= Welding length Unit: mm (in.)
- ( ): The number of welds

Construction

- Drill the welded flange of the roof panel and remove it.
- Check the front roof rail, the roof arch A, and the rear roof rail position for damage. If necessary, replace them.