( TL19E00D52100057091KBAT00 )

Steering Angle Sensor Replacement

NOTE:

- Do not damage or drop the combination switch as the steering angle sensor is sensitive to shock and vibration.
- The illustration shows LHD model, RHD model is symmetrical.

1. Remove the steering wheel.

1. Remove the steering column covers and the cable reel.

1. Remove the combination switch assembly.

1. Remove the combination light switch (A) and the wiper/washer switch (B) from the combination switch body assembly (C).

1. Install the combination switch body assembly in the reverse order of removal.
   NOTE:
   - Do not remove the steering angle sensor from the combination switch body.
   - When installing the cable reel, set the turn signal canceling sleeve position.
   - Note that the tightening order is specified for combination switch mounting screws.

NOTE:

- Do not damage or drop the combination switch as the steering angle sensor is sensitive to shock and vibration.
- The illustration shows LHD model, RHD model is symmetrical.

1. Remove the steering wheel.

1. Remove the steering column covers and the cable reel.

1. Remove the combination switch assembly.

1. Remove the combination light switch (A) and the wiper/washer switch (B) from the combination switch body assembly (C).

1. Install the combination switch body assembly in the reverse order of removal.
   NOTE:
   - Do not remove the steering angle sensor from the combination switch body.
   - When installing the cable reel, set the turn signal canceling sleeve position.
   - Note that the tightening order is specified for combination switch mounting screws.