( TL19E00J54260461997CBAT00 )

Fuse to Components Index - Passenger's Under-dash Fuse Holder

Passenger's Under-dash Fuse/Relay Box

Fuse Number | Amps | Component(s) or Circuit(s) Protected
--- | --- | ---
1 | 10 A | Passenger's MICU (H/L HI)
2 | 10 A | Passenger's MICU, Left front position light
3 | 10 A | Passenger's MICU, Left front fog light (LHD model), Right front fog light (RHD model)
4 | 15 A | Passenger's MICU (H/L LO)
5 | ——— | Not used
6 | 7.5 A | A/T gear position indicator panel light, Driver's seat heater switch light, Front passenger's seat heater switch light, Glove box light, Hazard warning switch light, Navigation display unit, VSA OFF switch light, Ashtray light, Cigarette lighter light, Headlight washer switch light, Headlight leveling switch light *1 , Driver's footwell light, Front passenger's footwell light, Front passenger's airbag cutoff switch light, Audio/navigation switch panel, Audio unit (without navigation), Heater control unit/climate control unit, Navigation unit (LHD model), Headlight washer and parking and back-up sensor switch light (LHD model), Center display unit (without navigation) (LHD model), Steering wheel switches lights (RHD model), Sunroof switch light/ambient light (RHD model), Ultrasonic off switch light (RHD model), Ultrasonic and inclination sensor off switch (RHD model), Parking and back-up sensor switch light (RHD model)
7 | ——— | Not used
8 | 20 A | Front passenger's power seat motors (recline, rear up-down)
9 | 20 A | Front passenger's power seat motors (slide, front up-down)
10 | 20 A *2 10 A *3 | Front passenger's door lock actuator, Passenger's MICU, Right rear door lock actuator (LHD model), Left rear door lock actuator (RHD model) Driver's super lock relay *2 , Passenger's super lock LOCK relay *2 , Passenger's super lock UNLOCK relay *2
11 | 20 A | Right rear power window switch (LHD model) *4 , Right rear power window switch (LHD model) *3 , Left rear power window switch (RHD model) *4 , Left rear power window switch (RHD model) *3 , Passenger's MICU
12 | 20 A | Accessory power socket
13 | 20 A | Front passenger's power window switch
14 | ——— | Not used
15 | 20 A | Stereo amplifier (with premium audio system)
16 | ——— | Not used
17 | 7.5 A | Passenger's MICU
18 | ——— | Not used
19 | 20 A | Driver's seat heater, Front passenger's seat heater
20 | 30 A (EPT R) | E-pretensioner unit
21 | 30 A (EPT L) | E-pretensioner unit
22 | ——— | Not used

*1: | Without headlight leveling system
*2: | KE model
*3: | Except KE model
*4: | With all power windows AUTO UP/AUTO DOWN function
*5: | Without all power windows AUTO UP/AUTO DOWN function