( TL19E00J26220219251KDAT10 )

Dashboard Side Vent Removal/Installation

1. Release the clips under the side vent (A).

   -1. | Insert a flat-tip screwdriver through a hole in the driver's side lid opening.
   -2. | While pushing on the inside clip (B) with a flat-tip screwdriver, carefully pull out the inside edge of the vent to release the upper tab (C).
   -3. | Repeat preceding step at the outside clip (D) and the upper tab (E).