CLUTCH RELEASE CYLINDER REMOVAL/INSTALLATION

#
CLUTCH RELEASE CYLINDER REMOVAL/INSTALLATION

B3E051041920W01

1. Remove the under cover.

2. Remove in the order indicated in the table.

3. Install in the reverse order of removal.

.

1 | Clutch pipe
2 | Bolt
3 | Clutch release cylinder

## Clutch Pipe Removal Note

1. Pull the clip to the position shown in the figure and pull out the clutch pipe connector straight to detach it.

F35M-R

G35M-R

## Clutch Pipe Installation Note

1. Return the clip to the position shown in the figure.

  Caution

  • Verify that there is no chipping or damage to the seal ring of the clutch pipe connector.

F35M-R

G35M-R

2. Insert the clutch pipe connector straight.

3. Pull the clutch pipe to verify that it does not come off, and reinsert it completely.