REAR WASHER NOZZLE REMOVAL/INSTALLATION

#
REAR WASHER NOZZLE REMOVAL/INSTALLATION

B3E091967511W01

1. Disconnect the negative battery cable.

2. Remove the liftgate upper trim. (SeeLIFTGATE UPPER TRIM REMOVAL/INSTALLATION.)

3. Remove the high-mount brake light. (SeeHIGH-MOUNT BRAKE LIGHT REMOVAL/INSTALLATION.)

4. Squeeze the tabs, then remove the rear washer nozzle.

5. Install in the reverse order of removal.

6. Adjust the rear washer nozzle. (See REAR WASHER NOZZLE ADJUSTMENT.)