CLIMATE CONTROL UNIT REMOVAL/INSTALLATION [FULL-AUTO AIR CONDITIONER]

#
CLIMATE CONTROL UNIT REMOVAL/INSTALLATION [FULL-AUTO AIR CONDITIONER]

B3E074061190W01

1.• Disconnect the negative battery cable.

2. Remove the ashtray panel. (See CONSOLE REMOVAL/INSTALLATION.)

3. Remove the decoration panel. (See DECORATION PANEL REMOVAL/INSTALLATION.)

4. Remove the center panel module. (See CENTER PANEL MODULE REMOVAL/INSTALLATION.)

5. Release the left and right tabs and remove as shown in the figure.

1 | Screw
2 | Climate control unit connector
3 | Climate control unit