FRONT FENDER PANEL REMOVAL/INSTALLATION

#
FRONT FENDER PANEL REMOVAL/INSTALLATION

B3E091052110W01

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Windshield wiper arm and blade (See WINDSHIELD WIPER ARM AND BLADE REMOVAL/INSTALLATION.)
  (2) Cowl grille (See COWL GRILLE REMOVAL/INSTALLATION.)
  (3) Front side turn lights (See FRONT SIDE TURN LIGHT REMOVAL/INSTALLATION.)
  (4) Front bumper (See FRONT BUMPER REMOVAL/INSTALLATION.)
  (5) Front combination lights (See FRONT COMBINATION LIGHT REMOVAL/INSTALLATION.)
  (6) Side step molding (Vehicle with the side step molding) (See SIDE STEP MOLDING REMOVAL/INSTALLATION.)

3. Remove in the order indicated in the table.

1 | Fastener
2 | Bolt A
3 | Bolt B
4 | Bolt C
5 | Bolt D
6 | Front fender panel

4. Install in the reverse order of removal.