DTC P0610 [LF]

#
DTC P0610 [LF]

B3E010201088W02

DTC P0610 | PCM vehicle options error
--- | ---
DETECTION CONDITION | • PCM data configuration error
POSSIBLE CAUSE | • Configuration procedure has not been completed • PCM malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY FREEZE FRAME DATA HAS BEEN RECORDED • Has FREEZE FRAME DATA been recorded? | Yes | Go to the next step.
No | Record the FREEZE FRAME DATA on the repair order, then go to the next step.
2 | VERIFY RELATED REPAIR INFORMATION AVAILABILITY • Verify related service repair information availability. • Is any related repair information available? | Yes | Perform repair or diagnosis according to the available repair information. • If the vehicle is not repaired, go to the next step.
No | Go to the next step.

3

VERIFY TROUBLESHOOTING OF DTC P0610 COMPLETED
• Make sure to reconnect all disconnected connectors.
• Turn the ignition switch to the ON position (Engine off).
• Clear the DTC from the PCM memory using the WDS or equivalent.
• Start the engine.
• Is the same DTC present?

Yes

Replace the PCM, then go to the next step.
(See PCM REMOVAL/INSTALLATION [LF].)

No | Go to the next step.
4 | VERIFY AFTER REPAIR PROCEDURE • Perform the "After Repair Procedure". (See AFTER REPAIR PROCEDURE [LF].) • Are any DTC present? | Yes | Go to the applicable DTC troubleshooting. (See DTC TABLE [LF].)
No | Troubleshooting completed.