POWER WINDOW MAIN SWITCH REMOVAL/INSTALLATION

#
POWER WINDOW MAIN SWITCH REMOVAL/INSTALLATION

B3E091266330W01

1. Disconnect the negative battery cable.

2. Remove clip B using a flathead screwdriver wrapped with protective tape.

3. Remove the switch panel from the front door trim while sliding it in the direction of the arrow as shown in the figure.

4. Disconnect the power window main switch connector and the power outer mirror switch connector.

5. Remove the screws, then remove the power window main switch.

6. Install in the reverse order of removal.