BATTERY RECHARGING

#
BATTERY RECHARGING

B3E011718520W04

  Warning

  • Keep all flames away from the battery, otherwise evaporated gas from the battery fluid may catch fire, and cause serious injury.
  • Remove the battery filler caps when recharging to prevent battery deformation or damage.

  Caution

  • Do not quick charge for over 30 min. It will damage the battery.

1. Remove the battery and then place it in a pan of water.

2. Connect a battery charger to the battery and adjust the charging current as follows.

Standard specification

Battery type (5-h rate) | Recharge current (A) | Quick charge (A/30 min)
--- | --- | ---
50D20L (40) | 4.0-5.0 | 25
75D26L (52) | 5.0-6.0 | 35
80D26L (55) | 5.5-6.5 | 35

3. After the battery is recharged, verify that the voltage is within the specification and remains at the same value for 1 h or more after the recharging was completed.

  • If not within the specification, replace the battery.

  Standard voltage
  12.4 V or more