TRANSAXLE RANGE (TR) SWITCH INSPECTION

#
TRANSAXLE RANGE (TR) SWITCH INSPECTION

B3E051719440W01

## Operating Inspection

1. Verify that the starter operates only when the ignition switch is turned to the START position with the selector lever in P or N position.

  • If there is any malfunction, adjust the TR switch.

2. Verify that the back-up lights illuminate when shifted to R position with the ignition switch at the ON position.

  • If there is any malfunction, adjust the TR switch.

3. Verify that the positions of the selector lever and the indicator are aligned.

  • If there is any malfunction, adjust the TR switch.

## Continuity Inspection

  Caution

  • Water or foreign material entering the connector can cause a poor connection or corrosion. Be sure not to drop water or foreign material on the connector when disconnecting it.

1. Remove the battery cover. (See BATTERY REMOVAL/INSTALLATION [ZJ, Z6].) (See BATTERY REMOVAL/INSTALLATION [LF].)

2. Disconnect the negative battery cable.

3. Remove the under cover.

4. Disconnect the TR switch connector.

5. Verify that the continuity is as indicated in the table.

  • If there is any malfunction, adjust the TR switch and go to Step 5.

6. Reinspect for continuity at TR switch.

  • If there is any malfunction, replace the TR switch. (See TRANSAXLE RANGE (TR) SWITCH REMOVAL/INSTALLATION.)

7. Connect the TR switch connector.

8. Install the under cover.

9. Connect the negative battery cable.

10. Install the battery cover. (See BATTERY REMOVAL/INSTALLATION [ZJ, Z6].) (See BATTERY REMOVAL/INSTALLATION [LF].)

## Resistance Inspection (On-Vehicle Inspection)

  Caution

  • Water or foreign material entering the connector can cause a poor connection or corrosion. Be sure not to drop water or foreign material on the connector when disconnecting it.

1. Remove the battery cover. (See BATTERY REMOVAL/INSTALLATION [ZJ, Z6].) (See BATTERY REMOVAL/INSTALLATION [LF].)

2. Disconnect the negative battery cable.

3. Remove the under cover.

4. Disconnect the TR switch connector.

5. Measure the resistance between the following terminals.

  • If there is any malfunction, inspect the ground, then perform the operating inspection.

Terminal | Position/Range | Resistance (ohm)
--- | --- | ---
B-C | P | 4,085-4,515
R | 1,425-1,575
N | 713-788
D | 371-409

6. Connect the TR switch connector.

7. Install the under cover.

8. Connect the negative battery cable.

9. Install the battery cover. (See BATTERY REMOVAL/INSTALLATION [ZJ, Z6].) (See BATTERY REMOVAL/INSTALLATION [LF].)