REAR DOOR SPEAKER REMOVAL/INSTALLATION

#
REAR DOOR SPEAKER REMOVAL/INSTALLATION

B3E092066961W03

1. Disconnect the negative battery cable.

2. Remove the rear door trim.(See REAR DOOR TRIM REMOVAL/INSTALLATION.)

3. Remove in the order indicated in the table.

1 | Screw
2 | Connector
3 | Rear door speaker (See Rear Door Speaker Installation Note.)

4. Install in the reverse order of removal.

## Rear Door Speaker Installation Note

1. Remove the speaker with the wiring harness passing through the groove of the rear door module.

  Caution

  • If the speaker is installed with the wiring harness out of the groove, an open circuit in the wiring harness could occur.