AIR MIX ACTUATOR REMOVAL/INSTALLATION

#
AIR MIX ACTUATOR REMOVAL/INSTALLATION

B3E074061415W01

1.• Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Front doors (See FRONT DOOR REMOVAL/INSTALLATION.)
  (2) Console (See CONSOLE REMOVAL/INSTALLATION.)
  (3) Shift lever component (MTX) (See SHIFT MECHANISM REMOVAL/INSTALLATION.)
  (4) Selector lever component (ATX) (See SELECTOR LEVER COMPONENT REMOVAL/INSTALLATION.)
  (5) Decoration panel (See DECORATION PANEL REMOVAL/INSTALLATION.)
  (6) Front scuff plate (See FRONT SCUFF PLATE REMOVAL/INSTALLATION.)
  (7) Front side trim (See FRONT SIDE TRIM REMOVAL/INSTALLATION.)
  (8) Glove compartment (See GLOVE COMPARTMENT REMOVAL/INSTALLATION.)
  (9) Shower ducts (LH, RH) (See A/C UNIT REMOVAL/INSTALLATION.)
  (10) PJB (See PASSENGER JUNCTION BOX (PJB) REMOVAL/INSTALLATION.)
  (11) Car-navigation unit (See CAR-NAVIGATION UNIT REMOVAL/INSTALLATION.)
  (12) Lower panel (See LOWER PANEL REMOVAL/INSTALLATION.)
  (13) Column cover (See COLUMN COVER REMOVAL/INSTALLATION.)
  (14) Meter hood (See METER HOOD REMOVAL/INSTALLATION.)
  (15) Instrument cluster (See INSTRUMENT CLUSTER REMOVAL/INSTALLATION.)
  (16) Steering shaft (See STEERING WHEEL AND COLUMN REMOVAL/INSTALLATION.)
  (17) A-pillar trim (See A-PILLAR TRIM REMOVAL/INSTALLATION.)
  (18) Center panel module (See CENTER PANEL MODULE REMOVAL/INSTALLATION.)
  (19) LCD unit (See LCD UNIT REMOVAL/INSTALLATION.)
  (20) Cowl grille (See COWL GRILLE REMOVAL/INSTALLATION.)
  (21) Cowl panel (See COWL PANEL REMOVAL/INSTALLATION.)
  (22) Windshield wiper arm and blade (See WINDSHIELD WIPER ARM AND BLADE REMOVAL/INSTALLATION.)
  (23) Windshield wiper motor (See WINDSHIELD WIPER MOTOR REMOVAL/INSTALLATION.)

3. Disconnect the air mix wire from the air mix link and wire clamp. (Manual air conditioner)

4. Disconnect the airflow mode wire from the airflow mode main link and wire clamp. (Manual air conditioner)

5. Disconnect the following connectors:

  - Blower motor connector
  - Power MOS FET connector (Full-auto air conditioner)
  - Evaporator temperature sensor connector
  - Air intake actuator connector
  - Air mix actuator connector (Full-auto air conditioner)
  - Airflow mode actuator connector (Full-auto air conditioner)

6. Remove the rear heat duct (1).

7. Remove the heater case. (See A/C UNIT REMOVAL/INSTALLATION.)

8. Remove the nuts and bolts for installing the dashboard to the body.

9. Remove in the air mix actuator.

.

1 | Air mix actuator connector
2 | air mix actuator

10. Install in the reverse order of removal.