AUDIO CONTROL SWITCH REMOVAL/INSTALLATION

#
AUDIO CONTROL SWITCH REMOVAL/INSTALLATION

B3E092000148W01

1. Disconnect the negative battery cable.

2. Remove the driver-side air bag module.(See DRIVER-SIDE AIR BAG MODULE REMOVAL/INSTALLATION.)

3. Remove the steering wheel.(See STEERING WHEEL AND COLUMN REMOVAL/INSTALLATION.)

4. Remove in the order indicated in the table.

.

1 | Cover
2 | Audio control switch (See Audio Control Switch Installation Note.)

5. Install in the reverse order of removal.

## Audio Control Switch Installation Note

1. Install the audio control switch so that the audio control switch wiring harness passes behind the steering wheel as shown in the figure.