REAR UPPER ARM REMOVAL/INSTALLATION

#
REAR UPPER ARM REMOVAL/INSTALLATION

B3E021428210W01

1. Remove the rear auto leveling sensor. (See AUTO LEVELING SENSOR REMOVAL/INSTALLATION.)

2. Remove in the order indicated in the table.

3. Install in the reverse order of removal.

4. Inspect the wheel alignment and adjust it if necessary.

(See REAR WHEEL ALIGNMENT.)

.

1 | Rear lower arm outer bolt (See Rear Lower Arm Outer Bolt Removal Note.)
2 | Rear coil spring component (See REAR COIL SPRING REMOVAL/INSTALLATION.)
3 | Rear upper arm (See Rear Upper Arm Installation Note.)

## Rear Lower Arm Outer Bolt Removal Note

1. Support the rear lower arm using a jack.

2. Loosen the rear lower arm inner bolt.

3. Remove the rear lower arm outer bolt.

## Rear Upper Arm Installation Note

1. Install the rear upper arm so that IN mark is facing toward the inside of the vehicle.