BRAKES

#
BRAKES

B3E045001020W01

Item | Specification
--- | ---
CONVENTIONAL BRAKE SYSTEM
Brake pedal | Pedal height (reference value) | (mm {in}) | 136.4 {5.37}
Pedal play | (mm {in}) | 4.0-8.4 {0.16-0.33}
Pedal-to-floor clearance (Brake pedal when depressed at 147 N {15.0 kgf, 33 lbf}) | (mm {in}) | 89.8 {3.54} or more
Power brake unit | Fluid pressure when pedal depressed at 200 N {20.4 kgf, 44.9 lbf} | At 0 kPa {0 mmHg, 0 inHg} | 500 {5.10, 72.6} or more
(kPa {kgf/cm2, psi}) | At 66.7 kPa {500 mmHg, 19.7 inHg} | 6,500 {66.29, 942.8} or more
Front brake (disc) | Minimum disc pad thickness | (mm {in}) | 2.0 {0.079}
Minimum disc plate thickness | (mm {in}) | 23 {0.91}
Disc plate runout limit | (mm {in}) | 0.05 {0.002}
Rear brake (disc) | Minimum disc pad thickness | (mm {in}) | 2.0 {0.079}
Minimum disc plate thickness | (mm {in}) | 9 {0.35}
Disc plate runout limit | (mm {in}) | 0.05 {0.002}
Brake fluid | Type | SAE J1703, FMVSS 116 DOT-3 or DOT-4
PARKING BRAKE SYSTEM
Parking brake lever | Lever stroke when pulled with 98 N {10 kgf, 22 lbf} at point 50 mm {1.97 in} from the end of the parking brake lever | (notches) | 3-6