DTC B2665

#
DTC B2665

B3E090200200W02

DTC B2665 | Battery back sounder circuit failure
--- | ---
DETECTION CONDITION | Short to power in wiring harness between PJB and theft-deterrent siren
POSSIBLE CAUSE | • Short to power supply in wiring harness between PJB terminal J-05 R and theft-deterrent siren terminal B • Theft-deterrent siren malfunction • PJB malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---

1

INSPECT THEFT-DETERRENT SIREN CONNECTOR
• Turn the ignition switch off.
• Disconnect the theft-deterrent siren connector.
• Inspect the theft-deterrent siren connector terminals for poor connection (such as damaged/pulled-out pins, and corrosion).
• Is there any malfunction?

Yes

Repair or replace the terminal, then go to Step 4.

No | Go to the next step.
2 | INSPECT PJB CONNECTOR • Disconnect the PJB connector. • Inspect the PJB connector terminals for poor connection (such as damaged/pulled-out pins, and corrosion). • Is there any malfunction? | Yes | Repair or replace the terminal, then go to Step 4.
No | Go to the next step.
3 | INSPECT THEFT-DETERRENT SIREN SIGNAL CIRCUIT FOR SHORT TO POWER SUPPLY • Turn the ignition switch to the ON position (Engine off). • Measure the voltage between PJB terminal J-05 R (wiring harness-side) and body GND. • Is the voltage B+? | Yes | Repair or replace the wiring harness for a possible short to power supply, then go to the next step.
No | Replace the theft-deterrent siren, then go to the next step. (See THEFT-DETERRENT SIREN REMOVAL/INSTALLATION [4SD], THEFT-DETERRENT SIREN REMOVAL/INSTALLATION [5HB].)
4 | VERIFY TROUBLESHOOTING COMPLETED • Make sure to reconnect all disconnected connectors. • Clear the DTC from the PJB memory using the WDS or equivalent. • Turn the ignition switch off then ON. • Is the same DTC present? | Yes | Replace the PJB. (See PASSENGER JUNCTION BOX (PJB) REMOVAL/INSTALLATION.)
No | DTC troubleshooting completed.