REAR DOOR TRIM REMOVAL/INSTALLATION

#
REAR DOOR TRIM REMOVAL/INSTALLATION

B3E09176852YW01

1. Disconnect the negative battery cable. (vehicle with power window system)

2. Using a small flathead screwdriver, open the cap and remove the screw, then remove the inner handle cover.

3. Remove the sail garnish. (5HB) (See SAIL GARNISH REMOVAL/INSTALLATION.)

4. Remove the regulator handle. (vehicle without power window system) (See REGULATOR HANDLE REMOVAL.) (SeeREGULATOR HANDLE INSTALLATION.)

5. Using a small flathead screwdriver, open the cap and remove the screw.

6. Detach clips A from the front door using a fastener remover.

7. Pull the rear door trim upward and detach tabs B from the rear door.

8. Disconnect the power window subswitch connector. (vehicle with power window system)

9. Remove the rear door trim.

10. Install in the reverse order of removal.