DSC SYSTEM INSPECTION

#
DSC SYSTEM INSPECTION

B3E041543000W02

## Preparation

1. Verify that the battery is fully charged.

2. Turn the ignition switch to the ON position and verify that the ABS warning light goes out after approx. 3.0 s.

3. Turn the ignition switch off.

4. Jack up the vehicle and support it evenly on safety stands.

5. Shift to the N position.

6. Verify that all four wheels rotate.

7. Rotate the inspected wheels by hand and verify there is no brake drag.

  • If there is any brake drag, perform regular brake inspection.
  • If there is no brake drag, perform DSC HU/CM operation inspection.

## ABS Control Inspection

1. Perform "Preparation".

2. Connect the WDS or equivalent to the DLC-2.

3. Set up an active command mode inspection according to the combination of commands below.

Brake pressure retention

Command name | Inspected wheels
--- | ---
LF | RF | LR | RR
LF_TC_PRV | OFF
RF_TC_PRV
LF_TC_SWV
RF_TC_SWV
LF_INLET | ON | OFF | OFF | OFF
LF_OUTLET | OFF
LR_INLET | ON
LR_OUTLET | OFF
RF_INLET | ON
RF_OUTLET | OFF
RR_INLET | ON
RR_OUTLET | OFF
PMP_MOTOR

Brake pressure reduction

Command name | Inspected wheels
--- | ---
LF | RF | LR | RR
LF_TC_PRV | OFF
RF_TC_PRV
LF_TC_SWV
RF_TC_SWV
LF_INLET | ON | OFF | OFF | OFF
LF_OUTLET
LR_INLET | OFF | ON
LR_OUTLET
RF_INLET | ON | OFF
RF_OUTLET
RR_INLET | OFF | ON
RR_OUTLET
PMP_MOTOR | ON

  Caution

  • When operating the solenoid valve and pump motor using the active command mode, make sure to keep the operation time within 2 s to prevent damaging the DSC HU/CM.

  Note

  • When working with two people, one should press on the brake pedal, the other should attempt to rotate the wheel being inspected.

4. Send the command while depressing on the brake pedal and attempting to rotate the wheel being inspected.

5. When brake pressure is maintained and a DSC HU/CM operation click sound is heard, confirm that the wheel does not rotate. When brake pressure is being reduced and a DSC HU/CM operation click sound is heard, confirm that the wheel rotates.

  • Performing the inspection above determines the following:

  - The DSC HU/CM brake lines are normal.
  - The DSC HU/CM hydraulic system has no significant malfunction (including DSC HU/CM).
  - The DSC HU/CM internal electrical parts (solenoid, motor and other parts) are normal.
  - The DSC unit and DSC HU/CM output system wiring harnesses (solenoid valve, relay system) are normal.

  • However, the following items cannot be verified.

  - Intermittent malfunction of the above items
  - Malfunction of DSC HU/CM input system wiring harnesses and parts
  - Extremely small leakage in the DSC HU/CM internal hydraulic system

## DSC Control Inspection

1. Perform "Preparation".

2. Connect the WDS or equivalent to the DLC-2.

3. Set up an active command mode inspection according to the combination of commands below.

  Caution

  • When operating the solenoid valve and pump motor using the active command mode, make sure to keep the operation time within 2 s to prevent damaging the DSC HU/CM.

Command name | Inspected wheels
--- | ---
Understeer control disabled | Oversteer control disabled
LF | RF | LR | RR
LF_TC_PRV | ON | OFF | ON
RF_TC_PRV | OFF | ON | OFF
LF_TC_SWV | OFF
RF_TC_SWV
LF_INLET | OFF | OFF | OFF | ON
LF_OUTLET | OFF
LR_INLET | ON
LR_OUTLET | OFF
RF_INLET | ON
RF_OUTLET | OFF
RR_INLET | ON
RR_OUTLET | OFF
PMP_MOTOR | ON

4. Send the command while rotating the wheel being inspected by hand in a forward direction.

5. Confirm that the wheel does not rotate easily while a DSC HU/CM operation click sound is heard.

  • Performing the inspection above determines the following:

  - The DSC HU/CM brake lines are normal.
  - The DSC HU/CM hydraulic system has no significant malfunction (including DSC HU/CM).
  - The DSC HU/CM internal electrical parts (solenoid, motor and other parts) are normal.
  - The DSC unit and DSC HU/CM output system wiring harnesses (solenoid valve, relay system) are normal.

  • However, the following items cannot be verified.

  - Intermittent malfunction of the above items
  - Malfunction of DSC HU/CM input system wiring harnesses and parts
  - Extremely small leakage in the DSC HU/CM internal hydraulic system