KEYLESS CONTROL MODULE INSPECTION

#
KEYLESS CONTROL MODULE INSPECTION

B3E091467820W02

1. Measure the voltage or inspect for continuity according to the Terminal Voltage Table (Reference).

  • If the voltage is not as specified in the Terminal Voltage Table (Reference), inspect the parts under "Inspection item(s)" and related wiring harnesses.

2. If the system does not work properly even though the inspection items or related wiring harnesses do not have any malfunction, perform symptom troubleshooting [KEYLESS ENTRY SYSTEM].

## Terminal Voltage Table (Reference)

Terminal | Signal name | Connected to | Measured condition | Voltage (V)/Continuity | Inspection item(s)
--- | --- | --- | --- | --- | ---
A | Power supply | PJB | Under any condition | B+ | • PJB (See PASSENGER JUNCTION BOX (PJB) INSPECTION.) • Related wiring harnesses
C | Data | PJB | Under any condition: Inspect the wiring harness between the keyless control module and PJB terminal J-04 F for continuity. | Continuity detected | • PJB (See PASSENGER JUNCTION BOX (PJB) INSPECTION.) • transmitter (See TRANSMITTER BATTERY INSPECTION.) • Related wiring harnesses
E | GND | Body ground | Under any condition: Inspect for continuity to ground. | Continuity detected | GND