THERMOSTAT INSPECTION [LF]

#
THERMOSTAT INSPECTION [LF]

B3E011215171W04

1. Inspect the thermostat for the following.

  Warning

  • During inspection, the thermostat and water are extremely hot and they can cause burns. Do not touch the thermostat and water.

  • The valve should not open under normal temperature.
  • Opening temperature and valve lift

  - If there is malfunction, replace the thermostat.

Item | Specification
--- | ---
Initial-opening temperature | (°C {°F}) | 80-84 {176-183}
Full-open temperature | (°C {°F}) | 97 {207}
Full-open lift | (mm {in}) | 8.0 {0.31} or more