IDLE AIR CONTROL (IAC) VALVE INSPECTION [ZJ, Z6]

#
IDLE AIR CONTROL (IAC) VALVE INSPECTION [ZJ, Z6]

B3E011320661W02

## Resistance Inspection

1. Disconnect the negative battery cable.

2. Disconnect the IAC valve connector.

3. Measure the resistance between IAC valve terminals A and B.

  • If within the specification, carry out the "Circuit Open/Short Inspection".
  • If not within the specification, replace the IAC valve.

  Resistance
  8.8-10.6 ohms [24°C {75 °F}]

## Circuit Open/Short Inspection

1. Inspect the following wiring harnesses for an open or short circuit. (Continuity check)

### Open circuit

  • If there is no continuity, the circuit is open. Repair or replace the wiring harness.
  - IAC valve terminal A and PCM terminal 2X
  - IAC valve terminal B and PCM terminal 2AB

### Short circuit

  • If there is continuity, the circuit is shorted. Repair or replace the wiring harness.
  - IAC valve terminal A and body GND
  - IAC valve terminal B and power supply