FRONT BUMPER REINFORCEMENT REMOVAL/INSTALLATION

#
FRONT BUMPER REINFORCEMENT REMOVAL/INSTALLATION

B3E091050070W01

1. Remove the front bumper. (See FRONT BUMPER REMOVAL/INSTALLATION.)

2. Remove the front combination light. (See FRONT COMBINATION LIGHT REMOVAL/INSTALLATION.)

3. Remove the horn. (SeeHORN REMOVAL/INSTALLATION.)

4. Set the following parts out of the way

  (1) Under cover
  (2) Electric power steering oil pump (LF)
  (3) Washer tank

5. Remon the order indicated in the table.

  Caution

  • If bolt A (only one location on the lower left) is removed, always replace it with the specialized replacement part (Part No. BPYK 50 0Z2) to ensure proper horn ground connection.

.

1 | Bolt A
2 | Bolt B
3 | Front bumper reinforcement (See Front Bumper Reinforcement Installation Note.)

6. Install in the reverse order of removal.

7. After installation, verify that the horn functions normally.

## Front Bumper Reinforcement Installation Note

### reusing the front bumper reinforcement

  Caution

  • In order to ensure proper body ground connection, do not apply paint in the area where the bolt A flange contacts the front bumper reinforcement.

### installing a new front bumper reinforcement

1. Remove the masking tape from the front bumper reinforcement.

  • If the masking tape has already peeled off, scrape off any rust or paint residue from the masked area.

2. After installing bolt A, apply touch-up paint to the area of the front bumper reinforcement that has remained unpainted.