A/C UNIT DISASSEMBLY/ASSEMBLY [FULL-AUTO AIR CONDITIONER]

#
A/C UNIT DISASSEMBLY/ASSEMBLY [FULL-AUTO AIR CONDITIONER]

B3E071161130W02

1. Disassemble in the order indicated in the table.

  Caution

  • If a non-specified grease is used, it may result in abnormal noise or improper operation of the links. Apply only the specified grease to each link.

2. Assemble in the reverse order of disassembly.

L.H.D.

R.H.D.

.

1 | Adhesive polyurethane (1)
2 | Blower case (1)
3 | Blower case (2)
4 | Air intake actuator
5 | Air intake link set
6 | Blower motor (See BLOWER MOTOR REMOVAL.) (See BLOWER MOTOR INSTALLATION.)
7 | Power MOS FET
8 | Air mix link set
9 | Air mix actuator
10 | Airflow mode link set
11 | Airflow mode main link
12 | Airflow mode actuator
13 | Polyurethane foam
14 | Adhesive polyurethane (2)
15 | Adhesive polyurethane (3)
16 | Adhesive polyurethane (4) (R.H.D.)
17 | Adhesive polyurethane (5) (R.H.D.)
18 | Evaporator pipe
19 | Expansion valve
20 | Adhesive polyurethane (6) (R.H.D.)
21 | Heater core
22 | Bracket (1)
23 | Bracket (2)
24 | Air filter
25 | A/C case (1)
26 | A/C case (2)
27 | Bolt (See Bolt Assembly Note.)
28 | Sensor clamp (See Sensor Clamp Assembly Note.)
29 | Evaporator temperature sensor (See Evaporator Temperature Sensor Assembly Note.)
30 | Evaporator
31 | A/C case (3)

## Evaporator Temperature Sensor Assembly Note

1. Assemble the evaporator temperature sensor as shown in the figure.

## Sensor Clamp Assembly Note

1. Attach the sensor clamp as shown in the figure.

## Bolt Assembly Note

1. Tighten it to the right so that it is flush to the contact surface.